|  |  |  |
| --- | --- | --- |
| jp801facejp801 | MOTOR | **Output: 2HP** |
| TABLE | Length: 1800mmWidth :230mm |
| CUTTERHEAD | Speed:4800r.p.m/50Hz 5900r.p.m/60HzNumber of knives:4Diameter:75mm |
| FENCE | Size: 1010x120mmTilt: 45ºin and out |
| CUTTING CAPATITY | Width: 200mmDepth: 3.175mmRabbeting:12.7mm |
| WEIGHT | N.W.: Body:141kg Stand:52kgG.W.:Body:155kgStand:54.5kg |
| PACKING MEASURE | Body:L1880xW440Xh270mmStand:L600xW470xH650mm |
|  |  |
|  |  |
|  |  |

8” JOINTER/JP801